This document describes the organization and use of the different directories and files:

Gearhead 32GPT requires a specific flange, as per combination with following motors:

2250...BX4, 2444...B, 26xx...C(X)R, 2214...BXT, 3216...BXT and 2264...BP4
please add 3D - file name: 32GPT_LN_flange_a

3242...CR, 3257...CR, 32xx...BX4 and AM3248...10
please add 3D - file name: 32GPT_LN_flange_b

3056...B
please add 3D - file name: 32GPT_LN_flange_c

3564...B
please add 3D - file name: 32GPT_LN_flange_d

3272...CR, 38xx...CR,  and 3274...BP4
please add 3D - file name: 32GPT_LN_flange_e

---------------------------------------------------------------------------------------------------
(c) Copyright 2025, DR.FRITZ FAULHABER GMBH & CO.KG.
All rights reserved.

